{"text_format":"1","workbook":"xlsx","n_sheets":25,"sheets":["Setting","0.Revision Note","1.Generalities","2.PLC Architecture","3.Panel Components","4.Control","5.Local Isolator","6.Field instruments","7.Process instruments","12.Local Isolator","13.Local Isolator - ATEX","16.PS & Transformer","17.PL & Transformer UL","18.MCC Panel","19.Local Boxes","20.Bus bar","21.Terminal Block","30.Burner","31.Burner Fiberizing","32.Burner SBM","40.Siemens-CPU","41.Siemens-ET200SP","42.Siemens-ET200SP DOL","60.Rockwell-CPU","61.Rockwell-Point IO"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":2,"defined_names":28,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Setting","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"cut":false,"hidden":false,"merged":[[2,1,2,5],[4,6,4,7],[1,6,1,9],[3,6,3,9],[0,6,0,8]]}
["TIPCHY73",null,null,null,null,null,"REVISION :",null,null,"Rev A"]
[null,null,null,null,null,null,"16.12.2025"]
[null,"PREFERRED ELECTRICAL EQUIPMENT/ SUPPLIERS"]
[null,null,null,null,null,null,"ISSUED BY : TIP Engineering"]
[]
[]
[null,"0. Lock / Unlock / Reset setting"]
[]
[]
[]
[]
[null,"1. Generalities"]
[]
[]
[]
[]
[null,"2. PLC Architecture"]
[]
[]
[]
[]
[null,"3. Panel Components"]
[]
[]
[]
[]
[null,"4. Power control"]
[]
[]
[]
[]
[null,"5. Local Isolator"]
[]
[]
[]
[]
[null,"6. Burner"]

{"sheet":"0.Revision Note","index":1,"n_rows":21,"n_cols":4,"rows_kept":21,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"Revision"]
[]
[]
[null,"Rev A","16.12.2025","First issue"]
[null,"Rev B"]
[null,"Rev C"]
[null,"Rev D"]
[null,"Rev E"]
[null,"Rev F"]
[null,"Rev G"]
[null,"Rev H"]
[null,"Rev I"]
[null,"Rev J"]
[null,"Rev K"]
[null,"Rev L"]
[null,"Rev M"]
[null,"Rev N"]
[null,"Rev O"]
[null,"Rev P"]

{"sheet":"1.Generalities","index":2,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[[0,1,0,5]]}
[null,"PLC Architecture"]
[]
["Filter","Designation",null,null,"Comments","Revision"]
[]
["Europe","Area","Europe",null,null,"A"]
["Asia",null,"Asia",null,null,"A"]
["USA",null,"USA",null,null,"A"]
["Canada",null,"Canada",null,null,"A"]
["Brasil",null,"Brasil",null,null,"A"]
["All"]
["All","Installation Standard"]
["Europe",null,"EN 60204-1:2024 - IEC60204",null,null,"A"]
["Asia",null,"EN 60204",null,null,"A"]
["USA",null,"EN 60204",null,null,"A"]
["Canada",null,"EN 60204",null,null,"A"]
["Brasil",null,"EN 60204",null,null,"A"]
["All"]
["All","Power Circuit","Neutral system ","TN-C",null,"A"]
["All"]
["Europe",null,"400V AC, 3 Phases, 50Hz",null,null,"A"]
["Asia",null,"400V AC, 3 Phases, 50Hz",null,null,"A"]
["USA",null,"480V AC, 3 Phases, 60Hz",null,null,"A"]
["Canada",null,"600V AC, 3 Phases, 60Hz",null,"460V AC for servo-motor","C"]
["Brasil",null,"400V AC, 3 Phases, 60Hz",null,null,"A"]
["All"]
["All","Control Circuit"]
["Europe",null,"Panel","24V DC","230VAC if 24VDC not available","A"]
["Europe",null,"Site","24V DC",null,"A"]
["Asia",null,"Panel","24V DC","230VAC if 24VDC not available","A"]
["Asia",null,"Site","24V DC",null,"A"]
["USA",null,"Panel","24V DC","120VAC if 24VDC not available","A"]
["USA",null,"Site","24V DC",null,"A"]
["Canada",null,"Panel","24V DC","120VAC if 24VDC not available","A"]
["Canada",null,"Site","24V DC",null,"A"]
["Brasil",null,"Panel","24V DC","230VAC if 24VDC not available","A"]
["Brasil",null,"Site","24V DC",null,"A"]
["All"]
["All","PLC Inputs / Outputs","24V DC",null,null,"A"]

{"sheet":"2.PLC Architecture","index":3,"n_rows":70,"n_cols":11,"rows_kept":70,"cut":false,"hidden":false,"merged":[[64,1,64,10],[34,1,34,10],[3,1,3,10],[30,2,33,2],[0,1,0,10],[8,1,8,10],[15,1,15,10],[21,1,21,10],[24,1,24,10],[26,1,26,10],[29,1,29,10]]}
[null,"PLC Architecture"]
[]
["Filter","Designation","Signal","Supplier","Reference / series","Comments","Link","Range","Remarks","Certification","Revision"]
["All","PLC "]
["Siemens","CPU",null,"Siemens","TIA 1500 Series",null,{"$error":"#VALUE!"},null,null,"CE / c-UL-us ","A"]
["Siemens","Distributed I/O","Profinet","Siemens","ET200SP",null,{"$error":"#VALUE!"},null,null,"CE / c-UL-us ","A"]
["Rockwell","CPU",null,"Rockwell","L8xS series",null,null,null,null,"see details","D"]
["Rockwell","Distributed I/O","Ethernet/IP","Rockwell","Point I/O",null,null,null,"- Exclusively over Ethernet/IP\n- Configuration to be validated with IAB Rockwell software","see details","D"]
["All","Process Network"]
["Siemens","Switch","Profinet","Siemens","6GK5208-0BA00-2AB2","SCALANCE XB-200 8 ports RJ",null,null,null,"CE / c-UL-us ","A"]
["Siemens","Switch","Profinet","Siemens","6GK5216-0BA00-2AB2","SCALANCE XB-200 16 ports RJ",null,null,null,"CE / c-UL-us ","A"]
["Siemens","Switch","Profinet","Siemens","6GK5213-3BB00-2AB2","SCALANCE XB-200 13 ports RJ + 3 ports Optic Fiber",null,null,"- when fiber optic link required","CE / c-UL-us ","A"]
["Siemens","PN/PN Coupler","Profinet","Siemens","6ES7158-3AD10-0XA0","Profinet / Profinet coupler",null,null,null,"CE / c-UL-us ","A"]
["Rockwell","Switch","Ethernet / IP","Rockwell","1783-CMS10B","Stratix 5200 - 8 copper / 2 ports Optic Fiber",null,null,null,"TBC","D"]
["Rockwell","Switch","Ethernet / IP","Rockwell","1783-CMS20DB","Stratix 5200 - 18 copper / 2 ports Optic Fiber",null,null,null,"TBC","D"]
["All","SCADA Network"]
["Siemens","Switch","Profinet","Siemens","6GK5216-4GS00-2AC2","SCALANCE XC216-4C G manageable  12x RJ45 PORTS 4x combo ports + C plug to add",null,null,null,"CE / c-UL-us ","A"]
["Siemens",null,null,"Siemens","6GK5992-1AG00-8AA0","SFP module",null,null,null,"CE / c-UL-us ","A"]
["Siemens",null,null,"Siemens","6GK1900-0AB10","C plug",null,null,null,"CE / c-UL-us ","A"]
["Siemens",null,null,null,null,null,null,null,null,"CE / c-UL-us ","A"]
["Rockwell","Switch","Ethernet / IP",null,null,"TBC confirmed according local architecture",null,null,null,"TBC","D"]
["Siemens","ProfiNet"]
["Siemens","Connector","Profinet","Siemens","6GK1901-1BB10-2AA0","180°",null,null,null,null,"A"]
["Siemens","Connector","Profinet","Siemens","6GK1901-1BB20-2AA0","90°",null,null,null,null,"A"]
["Rockwell","Ethernet/IP"]
["Rockwell","Connector","Ethernet/IP","Rockwell","1585J-M8CC-H","180°",null,null,null,"TBC","A"]
["Siemens","Profibus DP  "]
["Siemens","Connector","Profibus DP","Siemens","6ES7972-0BA52-0XA0","180°",null,null,null,null,"A"]
["Siemens","Connector","Profibus DP","Siemens","6ES7972-0BA61-0XA0","90°",null,null,null,null,"A"]
["All","Ethernet APL"]
["Siemens","Switch","APL","Pepper&Fuchs","ARS11-B2-IC08-2","Switch Ex ic 8 ports APL",null,null,null,null,"A"]
["Rockwell","Ethernet / IP - PA coupler",null,"APARIAN","ARS12-B2-IC16-1",null,null,null,null,"TBC","A"]
["Siemens",null,null,"Pepper&Fuchs","ARS12-B2-IC16-1","Switch Ex ic 16 ports APL",null,null,null,null,"A"]
["Siemens",null,null,"Pepper&Fuchs","ARS12-B2-IC24-1","Switch Ex ic 24 ports APL",null,null,null,null,"A"]
["All","Optic Fiber  "]
["All",null,null,"BELDEN","MIPP/AD/1S2P","MODULAR PATCH PANEL single module SC/SC Fiber adapter",null,null,"- For Profinet and Ethernet IP network",null,"A"]
["All",null,null,"GIGAMEDIA","GGM D5MLCLC3M","DUPLEX OPTICAL PATCHCORD LC/LC OM4 - LG : 3M",null,null,"- Patch cable between Patch panel and switch",null,"A"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"IO LINK"]
[null,"IO Link Head Module",null,"IFM","AL1304","HEAD MODULE 24VDC + PROFINET",null,null,null,null,"C"]
[null,"Bouchon M12",null,"IFM","E73004",null,null,null,null,null,"C"]
[null,"Ethernet/ProfiNet Connector Male Droit",null,"IFM","E12289",null,null,null,null,null,"C"]
[null,"M12 Plug Female supply Droit",null,"IFM","E11841",null,null,null,null,null,"C"]
[null,"IO LInk Connector Male Droit",null,"IFM","EVC816",null,null,null,null,null,"C"]

{"sheet":"3.Panel Components","index":4,"n_rows":56,"n_cols":10,"rows_kept":56,"cut":false,"hidden":false,"merged":[[0,1,0,9],[48,1,48,9],[36,1,36,9],[20,1,20,9],[27,1,27,9],[8,1,8,9],[3,1,3,9],[12,1,12,9],[13,1,13,9]]}
[null,"Panel Components"]
[]
["Filter ","Designation","Signal","Supplier","Reference / series","Comments","Link","Remarks","Certification\nCE / UL / CSA","Revision"]
["All","Terminal Blocks"]
["All","Main Supply Terminals",null,"nVent ERIFLEX","SBLL","250, 500 or 800amps",{"$error":"#VALUE!"},null,null,"A"]
["All","Motors Terminals",null,"PHOENIX CONTACT","PT","- Spring terminal up to 25mm²\n'- Feed-Through Terminal Block - PT",{"$error":"#VALUE!"},null,null,"A"]
["All","Motors Terminals",null,"nVent ERIFLEX","SB250","- 35 to 120mm²",{"$error":"#VALUE!"},null,null,"A"]
["All","Control Terminals",null,"PHOENIX CONTACT","QUATTRO / Twin",null,{"$error":"#VALUE!"},null,null,"A"]
["All","Main Switch  "]
["Schneider","Main switch (100 to 630 A)","400V AC","SCHNEIDER ELECTRIC","Compact NS___NA","- 3 Phases Main switch",null,null,null,"A"]
["Rockwell","Main switch (100 to 630 A)","400VAC to 600VAC","Rockwell","140G MOLDED CASE SWITCH","- 3 Phases Main switch",null,null,"TBC","A"]
["Rockwell","Main switch (30 to 600 A)","480VAC UL","Rockwell","194R NEMA J FUSED ","- 3 Phases Main switch",null,"Installation in US with Cable Operators\nand Operating Handles 194R-LFC03","TBC","F"]
["All","Control Circuit"]
["All","Power Supply"]
["Schneider","24V DC power supply","INPUT\n400 or 230V AC","Siemens","SITOP SMART",null,{"$error":"#VALUE!"},null,null,"A"]
["Schneider","24V DC UPS for PLC panel",null,"Siemens","6EP1933-2EC41",null,{"$error":"#VALUE!"},null,null,"A"]
["Schneider","230V AC Transformer",null,"Siemens","TRANSFORMER SITAS",null,{"$error":"#VALUE!"},null,null,"A"]
["Rockwell","24V DC power supply","INPUT\n120 / 230V AC","Rockwell","1606 XLS",null,null,null,"see details","A"]
["Rockwell","24V DC UPS for PLC panel",null,"Rockwell","1606 XLS",null,null,null,"see details","A"]
["Rockwell","230V AC Transformer",null,"Rockwell","1497B",null,null,null,"see details","A"]
["All","Circuit breaker"]
["Schneider","24V DC protection : Electronic Breaker - 0,5 to 3A","24V DC","Siemens","6EP1961-2BA11",null,null,null,null,"A"]
["Schneider","24V DC protection : Electronic Breaker - 3 to 10A","24V DC","Siemens","6EP1961-2BA21",null,null,null,null,"A"]
["Schneider","230V AC protection","230V AC","SCHNEIDER ELECTRIC","Acti9 i C60N",null,null,null,null,"A"]
["Rockwell","24V DC protection : Electronic Breaker - 1 to 6A","24V DC","MURR ELEKTRONIK"," 9000-41034-0100600","- to mitigate potential long lead time, SG-TIP recommands using \nRockwell  1489-M unipolar series for UL & CSA\nRockwell 1495-SP unipolar series for CEI",null,null,null,"A"]
["Rockwell","24V DC protection : Electronic Breaker - 4 to 10A","24V DC","MURR ELEKTRONIK","9000-41034-0401000","- to mitigate potential long lead time, SG-TIP recommands using \nRockwell  1489-M unipolar series for UL & CSA\nRockwell 1495-SP unipolar series for CEI",null,null,null,"A"]
["Rockwell","230V AC protection","120 / 230V AC","Rockwell",1489,null,null,null,null,"A"]
["All","Relays"]
["Schneider","Relays",null,"SCHNEIDER ELECTRIC","CAD","Coil 24VDC",null,null,null,"A"]
["Schneider","Relays Interface output 24VDC",null,"SCHNEIDER ELECTRIC","RXM4AB1BDPVS","Coil 24VDC",null,null,null,"A"]
["Schneider","Volt control relays",null,"SCHNEIDER ELECTRIC","RM17TG20","Adapt to local voltage reference",null,null,null,"A"]
["Schneider","Static Relays Coil for Brake",null,"SCHNEIDER ELECTRIC","SSM1A112BD","Coil 24VDC",null,null,null,"A"]
["Rockwell","Relays",null,"Rockwell","700-CF","Coil 24VDC",null,null,null,"A"]
["Rockwell","Relays SAFE signal",null,"Rockwell","700-S","Coil 24VDC",null,null,null,"A"]
["Rockwell","Relays Interface output 24VDC",null,"Rockwell","700-HLT12Z24","Coil 24VDC",null,null,null,"A"]
["Rockwell","Volt control relays",null,"Rockwell","813S-V3-400V for 400V\n813S-V3-480V for 480V\n813S-V3-690V for 600V","Adapt to local voltage reference",null,null,null,"A"]
["All","Accessories : push button, lamp, contol box…"]
["Schneider","Control buttons on panel",null,"SCHNEIDER ELECTRIC","XB4-B","Diameter 22,5 mm",null,null,null,"A"]
["Schneider","Indicator lamps on panel",null,"SCHNEIDER ELECTRIC","XB4-B","Diameter 22,5 mm",null,null,null,"A"]
["Schneider","Lighting columns",null,"SCHNEIDER ELECTRIC","XVB-C",null,null,null,null,"A"]
["Schneider","Operator control box  +\n Control buttons / indicator lamps",null,"SCHNEIDER ELECTRIC","XALD + XB5",null,null,null,null,"A"]
["Schneider","Emergency stop box",null,"SCHNEIDER ELECTRIC","XALK178F +ZBZ1605",null,null,null,null,"A"]
["Rockwell","Control buttons on panel",null,"Rockwell","800FM","Diameter 22,5 mm",null,null,null,"A"]
["Rockwell","Indicator lamps on panel",null,"Rockwell","800FM","Diameter 22,5 mm",null,null,null,"A"]
["Rockwell","Lighting columns",null,"Rockwell","855T",null,null,null,null,"A"]
["Rockwell","Operator control box  +\n Control buttons / indicator lamps",null,"Rockwell","FM800F + 800",null,null,null,null,"A"]
["Rockwell","Emergency stop box",null,"Rockwell","800F-1YM3 + 800F-A6PR5",null,null,null,null,"A"]
["All","Pre-start warning / Default warning",null,"ALLEN BRADLEY","855H-BD30CD","- 24VDC\n- 2 different sounds (one for pre-start warning, one for alarm)",null,null,null,"A"]
["All","MCC panels and remote IO boxes (CRB)"]
["All","Process Electrical Panels",null,"RITTAL","VX25","- Depth 600mm\n- Height 2000mm + plinth 200mm\n- Width 1200",{"$error":"#VALUE!"},null,"see details","A"]
["All","PLC Panel",null,"RITTAL","VX25","- Depth 600mm\n- Height 2000mm + plinth 200mm\n- Width 600",{"$error":"#VALUE!"},null,"see details","A"]
["All","Network / IT panels",null,"RITTAL","VX25","- Depth 600mm\n- Height 2000mm + plinth 200mm\n- Width 600",{"$error":"#VALUE!"},null,"see details","A"]
["All","Remote I/O box (CRB)",null,"RITTAL","KX or AX depending the size","- Size should be choice according the number of I/O cards",{"$error":"#VALUE!"},null,"see details","A"]
["All","Operator Panel",null,"RITTAL","one-piece TP if less 1200mm Width\n or Topconsole system TP above 1200mm width","- Depending the size",null,null,null,"A"]
["All","Cooling Unit",null,"RITTAL","Wall-mounted cooling unit","- Blue e+",null,"Power according the materials power loss",null,"A"]
["All","Power Bus Bar",null,"RITTAL","Busbar Rline",null,{"$error":"#VALUE!"},null,null,"A"]

{"sheet":"4.Control","index":5,"n_rows":28,"n_cols":10,"rows_kept":28,"cut":false,"hidden":false,"merged":[[0,1,0,9],[21,1,21,9],[3,1,3,9],[10,1,10,9]]}
[null,"Power Control"]
[]
["Filter","Designation","Supplier","Technology","Communication","Comments","Link","Remarks","Certification\nCE / UL / CSA","Revision"]
["All","DOL Starter"]
["Siemens","Direct On Line (DOL) / Reverse On Line (ROL) for standard application with standard and fail safe control","Siemens","ET200SP motor starter","Profinet","- use for motors up to 4 kW (9A)",{"$error":"#VALUE!"},null,null,"A"]
["Siemens","Direct On Line (DOL) / Reverse On Line (ROL) for standard application with standard and fail safe control","SCHNEIDER ELECTRIC","GV2-P + LC1-D",null,"- use for motors above 4 kW and up to 30 kW\n- Coil in 24V DC",null,null,null,"A"]
["Siemens/Schneider","Direct On Line (DOL) / Reverse On Line (ROL) for standard application with standard and fail safe control","SCHNEIDER ELECTRIC","GV2-P + LC1-D",null," - Up to 30 kW\n- Coil in 24V DC",null,null,null,"A"]
["Siemens/Schneider","Direct On Line (DOL) / Reverse On Line (ROL) for fans application with standard and fail safe control","SCHNEIDER ELECTRIC","GV2-L + LC1-D + LRD..L",null,"- For fans and motors starting in more than 10s.\n- class 20 motor starter\n- Up to 30 kW\n- Coil in 24V DC",null,null,null,"A"]
["Rockwell","Direct On Line (DOL) / Reverse On Line (ROL) for standard application with standard and fail safe control","Rockwell","14MT + 100-C","N/A",null,null,null,"see details","A"]
["Rockwell","Direct On Line (DOL) / Reverse On Line (ROL) for fans application with standard and fail safe control","Rockwell","140MT + 100-C + 193-EE","N/A","- For fans and motors starting in more than 10s.\n- class 20 motor starter\n- Up to 30 kW\n- Coil in 24V DC",null,null,"see details","A"]
["All","VFD"]
["Siemens","Frequency inverters ","Siemens","Sinamics G120C","Profinet","- for standard applications\n- motor power up to 132 kW",null,null,null,"A"]
["Siemens","Frequency inverters ","Siemens","Sinamics G120","Profinet","- for standard applications with encoder\n- motor power up to 110 kW",null,null,null,"A"]
["Siemens","Frequency inverters ","Siemens","Sinamics S120","Profinet","- for technology applications",null,"Mandatory: configuration to be done withe software \"SIZER\"   ",null,"A"]
["Siemens","Frequency inverters","Siemens","Sinamics G120P","Profinet","- for standard applications\n- only for motor power > 132 kW",null,null,null,"A"]
["Siemens","Frequency inverters","Siemens","Sinamics G150","Profinet","- for standard applications\n- only for motor power > xxx kW",null,null,null,"A"]
["Rockwell","Frequency inverters","Rockwell","Power Flex 525","Ethernet / IP","- for standard applications\n- motor power up to 30 HP (22 kW)",null,null,"CE / c-UL-us","D"]
["Rockwell","Frequency inverters ","Rockwell","Power Flex 753","Ethernet / IP","- for standard applications\n- motor power from 40 HP to 400 HP (30 to 300 kW)",null,null,"CE / c-UL-us","D"]
["Rockwell","Frequency inverters ","Rockwell","Power Flex 755","Ethernet / IP","- for standard applications\n- motor power above 400 HP (300 kW)",null,null,"CE / c-UL-us","D"]
["Rockwell","Frequency inverters ","Rockwell","Kinetix","Ethernet / IP","- for technology applications",null,"Mandatory: configuration to be done with software \"???\"   ","see details","A"]
["Schneider","Frequency inverters","SCHNEIDER ELECTRIC","ATV 900","Profinet","TBC",null,null,"see details","A"]
["All","Soft starter"]
["Siemens","AC soft starters","Siemens","3RW55..","Profinet","- for power motor > 37 kW ",null,null,null,"A"]
["Siemens","Safe AC soft starters","Siemens","3RW55..","Profinet","- for power motor > 37 kW ",null,null,null,"A"]
["Rockwell","AC soft starters","Rockwell","SMC","Ethernet / IP","- for power motor > 37 kW ",null,null,"see details","A"]
["Rockwell","Safe AC soft starters","Rockwell","SMC","Ethernet / IP","- for power motor > 37 kW ",null,null,"see details","A"]
["Schneider","AC soft starters","SCHNEIDER ELECTRIC",null,"Profinet","TBC","TBC",null,"see details","A"]
["Schneider","Safe AC soft starters","SCHNEIDER ELECTRIC",null,"Profinet","TBC","TBC",null,"see details","A"]

{"sheet":"5.Local Isolator","index":6,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[[13,1,13,8],[0,1,0,8],[3,1,3,8]]}
[null,"Local Isolators"]
[]
["Filter","Designation","Supplier","Series","Comments","Link","Remarks","Certification\nCE / UL / CSA","Revision"]
["All","Standard Application"]
["Kraus","Motor local isolator","KRAUS & NAIMER ","KGxxx T103/40 KLx1V",null,{"$error":"#VALUE!"},null,null,"A"]
["Kraus","Forward Jog Test Push Button","SCHNEIDER ELECTRIC","XB4BA21",null,null,null,null,"A"]
["Kraus","Forward and Backward Jog Test Push Button","SCHNEIDER ELECTRIC","XB4BD53",null,null,null,null,"A"]
["UL-CSA","Motor local isolator","Rockwell","194E",null,null,null,"see details","A"]
["UL-CSA","Jog Test Push Button","SCHNEIDER ELECTRIC","800FM-F2MX10",null,null,null,"TBC","A"]
["UL-CSA","Jog Test Push Button","SCHNEIDER ELECTRIC","800FM-F2MX10",null,null,null,"TBC","A"]
["Square D","Motor local isolator","SCHNEIDER ELECTRIC",null,null,null,null,"see details","D"]
["Square D","Jog Test Push Button","SCHNEIDER ELECTRIC",null,null,null,null,"TBC","D"]
["Square D","Jog Test Push Button","SCHNEIDER ELECTRIC",null,null,null,null,"TBC","D"]
["All","ATEX"]
["Kraus","Motor local isolator","KRAUS & NAIMER ","KG20 T203/NL-EXRA KNBOX",null,{"$error":"#VALUE!"},null,null,"A"]
["Kraus","Forward Jog Test Push Button","STAHL","8040/1180X-01L50BA05",null,null,null,null,"A"]
["Kraus","Forward and Backward Jog Test Push Button","STAHL",null,null,null,null,null,"A"]
["UL-CSA","Motor local isolator","CROUSE-HINDS","GHG",null,null,null,"see details","A"]
["UL-CSA","Jog Test Push Button","Rockwell","800G-1F2A3",null,null,null,"TBC","A"]
["UL-CSA","Forward and Backward Jog Test Push Button","Rockwell","TBC",null,null,null,"TBC","A"]
["Square D","Motor local isolator","SCHNEIDER ELECTRIC",null,null,null,null,"see details","D"]
["Square D","Jog Test Push Button","SCHNEIDER ELECTRIC",null,null,null,null,"TBC","D"]
["Square D","Jog Test Push Button","SCHNEIDER ELECTRIC",null,null,null,null,"TBC","D"]

{"sheet":"6.Field instruments","index":7,"n_rows":20,"n_cols":10,"rows_kept":20,"cut":false,"hidden":false,"merged":[[17,1,18,1],[5,1,7,1],[5,2,7,2],[9,2,10,2],[9,1,10,1],[0,1,0,9],[11,3,13,3],[9,3,10,3],[5,3,7,3],[15,3,16,3],[15,1,16,1],[11,1,14,1],[11,2,14,2]]}
[null,"Field Instrumentation"]
[]
["Filter","Designation","Signal","Supplier","Reference","Comments","Details","Remarks","Certification","Revision"]
["All","Solenoid valves",null,null,null,null,null,"Preferred 24VDC (max 0,5A)\n230VAC otherwise","CE ","A"]
["All","Rotation controllers","24VDC","IFM","DI6004",null,null,"M18, 3 wires","CE / c-UL-us ","A"]
["All","Inductive position switches","24VDC","IFM","IG 5846","M18",null,"4 wires (provides NO and NC contacts)","CE ","A"]
["All",null,null,null,"IG510A","M18 Ex",null,"3 wires. For Atex areas","CE ","A"]
["All",null,null,null,"II5785","M30",null,"3 wires","CE / c-UL-us ","A"]
["All","Inductive position switches SIL2","24VDC","IFM","GG712S",null,null,"2 outputs","CE / c-UL-us ","A"]
["All","Capacitive position switches","24VDC","IFM"," M18x1",null,null,"3 wires","CE ","A"]
["All",null,null,null,"M30x1, 5",null,null,null,"CE ","A"]
["All","Opto-electronic sensors","24VDC","LEUZE","HT46CI/4P-M12","Infrared",null,"Product positionning","CE / c-UL-us ","A"]
["All",null,null,null,"PRK 46B/66-S12","reflex",null,"Board positionning in turnover arms","CE / c-UL-us ","A"]
["All",null,null,null,"HRT 96M/P-1636-800-41","infrared\nHeated lense",null,"Board detection dryer inlet. \nLess sensitive to steam environments","CE / c-UL-us ","A"]
["All",null,null,"IFM","OG5119","optical sensor with background suppression",null,"Board detection in dryer outfeed\nambient temperature up to 80°C, range limited to 130mm, not infrared","CE ","A1"]
["Siemens","Absolute encoder","ProfiNet","TR","CEV58M","24VDC",null,null,"CE ","A"]
["Rockwell",null,"Ethernet / IP",null,"TBC",null,null,null,"TBC"]
["All","Emergency pull wires",null,"Telemecanique","XY2-CE1",null,null,"pull-wire length limited to 50m","CE ","A"]
["All",null,null,"Kiepe","HEN-002",null,null,"preferred\npull-wire length up to 100m","CE ","A"]
["All","Belt tracking switches","24VDC","Kiepe","MAS-001",null,null,"contact 1: 10 degree warning\nContact 2: 18 degree Alarm","CE ","A"]

{"sheet":"7.Process instruments","index":8,"n_rows":44,"n_cols":11,"rows_kept":44,"cut":false,"hidden":false,"merged":[[0,1,0,10],[10,1,11,1]]}
[null,"Process Instrumentation"]
[]
["Filter","Designation","Signal","Supplier","Reference","Comments","Range","Details","Remarks","Certification","Revision"]
["All","Level switches Gypsum","24VDC","Endress & Hauser","Solicap FTI5x / Minicap FTC26x",null,null,null,"Electronic: FEI52 (3 wire PNP)",null,"A"]
["All","Level switches stucco & Dry Adds","24VDC","Endress & Hauser","Soliphant M-FTMxx\nSoliphant T-FTM21","M = tuning fork\nT = rod",null,null,"Electronic: FEM22 (3 wire PNP)",null,"A"]
["All","Vibratory level switches (Liquids)","24VDC","Endress & Hauser","Liquiphant M \nFTL 31(compact) or\nFTL51","24VDC",null,null,"Electronic FEL52",null,"A"]
[null,"Temperature","RTD","Endress & Hauser","iTherm Module Line TM131 series",null,null,null,"no transmitter to be installed / sensor connected directly to IO RTD modules ",null,"B"]
["All","Radar level transmitters","ProfiNet over Ethernet APL","Endress & Hauser","DELTAPILOT","24 VDC (supply)",null,null,null,null,"A"]
["All","Ultrasonic level transmitters","ProfiNet over Ethernet APL","Endress & Hauser","Prosonic T FMU","24 VDC (supply)",null,null,null,null,"A"]
["All","Level Transmitters  (Pressure based)","ProfiNet over Ethernet APL","Endress & Hauser","DELTAPILOT  S","24 VDC (supply)",null,null,null,null,"A"]
["All","Load cells",null,"Sartorius / Minebea Intec"," PR6201 - PR6251","compression load cells",null,null,"No transmitter required / direct connection to IO module",null,"A"]
["All",null,null,"Sartorius / Minebea Intec","PR6130/64S","Junction box",null,null,null,null,"A"]
["Siemens","Weight Transmitter",null,"Siemens","7MH4138-6BA00-0CU0","Siwarex WP351",null,null,"load cells connected to ET200SP siwarex",null,"A"]
["Rockwell","Weight Transmitter",null,"Hardy","HI 1734-WS"," Point I/O Weight Processing Module",null,null,"load cells connected to PointIO module","TBC","B"]
["All","Fan bearing temperature transmitter","IO Link","IFM","TA2135","compact / M12 ",null,null,null,null,"A"]
["All","Pressure Transmitters","ProfiNet over Ethernet APL","Endress & Hauser","Cerabar S PMC71 B","24 VDC (supply)\nM12 connectors",null,null,null,null,"A"]
["All","Differential Pressure Transmitters","ProfiNet over Ethernet APL","Endress & Hauser","Deltabar PMD75 B","M12 connectors",null,null,null,null,"A"]
["Siemens","Magnetic flow meters (liquids)","Profinet","Endress & Hauser","Promag ",null,null,null,null,null,"A"]
["Rockwell","Magnetic flow meters (liquids)","Ethernet/IP","Endress & Hauser","Promag ",null,null,null,null,"TBC","A"]
["Siemens","Mass flow meters (liquids)","Profinet","Endress & Hauser","Promass ",null,null,null,null,null,"A"]
["Rockwell","Mass flow meters (liquids)","Ethernet/IP","Endress & Hauser","Promass ",null,null,null,null,"TBC","A"]
["Siemens","Air  flow meters (foam air)","Profinet","Endress & Hauser","Promass ",null,null,null,null,null,"A"]
["Rockwell","Air  flow meters (foam air)","Ethernet/IP","Endress & Hauser","Promass ",null,null,null,null,"TBC","A"]
["All","Vibration transmitter for large fan","IO Link","IFM","VVB001","24 VDC (supply)\ncompact\nM12",null,null,null,null,"A"]
["All","Air Humidity transmitter","24 VDC (supply), 4..20 mA (signal).","Vaisala","Indigo 520",null,"0..1000 g/kg and 0..100°C",null,"Wire sensor high temperature contact to PLC espacially when cooling fins removed.",null,"A"]
["All","Board Moisture transmitter","230 VAC (supply), 4..20 mA (signal).","Sensortech","ST-3300A",null,"0..100%",null,"Use 48\" high temperature version for in-kiln installation. Use 12\" low temperature version for Take Off installation.",null,"A"]
["All","Board Temperature transmitter","24 VDC (supply), 4..20 mA (signal).","Raytek","RDMI310LTSCB3 + MI3COMM","Compact MI3, LT sensing head.",null,null,"By default 1m sensor provided so order longer cable as per installation requirements.",null,"A"]
["Siemens","Dryer Damper Actuator","Profinet","Auma","SQRV or SARV","SQR (up to its torque limit), SAR otherwise ",null,null,null,null,"A"]
["Rockwell",null,"Ethernet / IP","Auma","SQR or SAR","SQR (up to its torque limit), SAR otherwise ",null,null,null,"TBC","A"]
["All","Air actuated Damper","Profibus PA","Siemens","Sipart PS2",null,null,null,null,null,"A"]
["All","Compressed Air Flow","24 VDC (supply), 4..20 mA (signal).","Endress & Hauser","Prowhirl 200",null,null,null,"Used for utility system measurement of compressed air flow for energy management.",null,"A"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Weigh Belt Feeder","ProfiNet","Kukla","DWC-7 series",null,null,null,null,null,"B"]

{"sheet":"12.Local Isolator","index":9,"n_rows":21,"n_cols":8,"rows_kept":21,"cut":false,"hidden":false,"merged":[[6,3,20,3],[6,5,20,5],[6,1,20,1],[2,2,4,2],[2,1,4,1],[3,0,4,0],[2,7,4,7],[2,3,2,6],[3,3,3,4],[3,5,3,6],[0,0,0,6]]}
["Local Isolators - Standard application",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[]
["Motor Power (kW)","Supplier","Reference","Jog Test",null,null,null,"Revision"]
["(Normal Duty)",null,null,"Forward",null,"Forward & Backward"]
[null,null,null,"Supplier","Reference","Supplier","Reference"]
["400VAC"]
[0.55000000000000004,"Kraus & Neimer","KG20 T203/F-A006 KL11V","SCHNEIDER ELECTRIC","XB4BA21","SCHNEIDER ELECTRIC","XB4BD53","A"]
[0.75,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[1.1000000000000001,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[1.5,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[2.2000000000000002,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[3,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[4,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[5.5,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[7.5,null,"KG20 T203/F-A006 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[11,null,"KG32 T203/F-A003 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[15,null,"KG41 T203/40 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[18.5,null,"KG64 T203/40 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[22,null,"KG64 T203/40 KL11V",null,"XB4BA21",null,"XB4BD53","A"]
[30,null,"KG80 T203/40 KL71V",null,"XB4BA21",null,"XB4BD53","A"]
[37,null,"KG100 T203/40 KL51V",null,"XB4BA21",null,"XB4BD53","A"]

{"sheet":"13.Local Isolator - ATEX","index":10,"n_rows":19,"n_cols":8,"rows_kept":19,"cut":false,"hidden":false,"merged":[[5,1,18,1],[5,3,18,3],[5,5,18,5],[2,7,4,7],[2,1,4,1],[2,2,4,2],[2,3,2,6],[3,0,4,0],[3,3,3,4],[3,5,3,6],[0,0,0,6]]}
["Local Isolators - ATEX",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[]
["Motor Power (kW)","Supplier","Reference","Jog Test",null,null,null,"Revision"]
["(Normal Duty)",null,null,"Forward",null,"Forward & Backward"]
[null,null,null,"Supplier","Reference","Supplier","Reference"]
[0.55000000000000004,"Kraus & Neimer","KG20 T203/NL-EXRA KNBOX","Stahl","8040/1180X-01L50BA05","Stahl","TBC","A"]
[0.75,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[1.1000000000000001,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
["400VAC"]
[1.5,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[2.2000000000000002,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[3,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[4,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[5.5,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[7.5,null,"KG20 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[11,null,"KG32 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[15,null,"KG41 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[18.5,null,"KG64 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]
[22,null,"KG64 T203/NL-EXRA KNBOX",null,"8040/1180X-01L50BA05",null,"TBC","A"]

{"sheet":"16.PS & Transformer","index":11,"n_rows":14,"n_cols":6,"rows_kept":14,"cut":false,"hidden":false,"merged":[[10,1,13,1],[4,4,6,4],[3,0,3,5],[4,1,8,1],[4,3,6,3],[9,0,9,5],[0,0,0,4]]}
["Power Supply & Transformer",null,null,null,null,{"$error":"#VALUE!"}]
[]
["Designation","Supplier","Reference","Remark","Comment","Revision"]
["Power Supply"]
["SUPPLY SITOP SMART 3 phases 400VAC/24VDC 10A","Siemens","6EP1434-2BA20","Protection with GV2RT07/08",null,"A"]
["SUPPLY SITOP SMART 3 phases 400VAC/24VDC 20A",null,"6EP1436-2BA10",null,null,"A"]
["SUPPLY SITOP SMART 3 phases 400VAC/24VDC 40A",null,"6EP1437-2BA40",null,null,"A"]
["SUPPLY SITOP SMART 1 Phase 110-220VAC/24VDC 10A",null,"6EP1334-2AA01-0AB0"," CHANGE FOR 6EP1334-2BA20 ??",null,"A"]
["UPS 24VDC SITOP 15A",null,"6EP1933-2EC41",null,null,"A"]
["Transformer"]
["1 phase 400V/230V 1000VA","Siemens","4AM5742-5AT10-0FA0","Protection with  GV2RT08",null,"A"]
["1 phase 400V/230V 1600VA",null,"4AM6142-5AT10-0FA0","Protection with  GV2RT10",null,"A"]
["1 phase 400V/230V 2000VA",null,"4AM6442-5AT10-0FA0","Protection with  GV2RT14",null,"A"]
["1 phase 400V/230V 2500VA",null,"4AM6542-5AT10-0FA0","Protection with  GV2RT14",null,"A"]

{"sheet":"17.PL & Transformer UL","index":12,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":true,"merged":[[0,0,0,5],[3,0,3,5],[5,1,8,1],[5,3,8,3],[15,0,15,5],[4,0,4,5],[9,0,9,5],[10,1,14,1],[10,3,14,3],[26,1,28,1],[20,0,20,5],[25,0,25,5],[16,1,19,1],[16,3,19,3],[21,3,24,3],[26,3,28,3],[21,1,24,1]]}
["Power Supply & Transformer"]
[]
["Designation","Supplier","Reference","Remark","Comment","Revision"]
["Power Supply"]
["400-480VAC Primary"]
["3 phases 380-480VAC / 24VDC 10A","Rockwell","1606-XLE240E-3","- protection with 140MT\n- to be defined according the input voltage",null,"A"]
["3 phase 380-480VAC / 24VDC 40A",null,"1606-XLS960E",null,null,"A"]
["UPS 24VDC ",null,"1606-XLS240-UPS",null,null,"A"]
["Battery",null,"1606-XLSBATASSY2",null,null,"A"]
["600VAC Primary"]
["1 phase 120/230VAC / 24VDC 10A","Rockwell","1606-XLS240E","- protection with 140MT\n- to be defined according the input voltage",null,"A"]
["1 phase 120/230VAC / 24VDC 20A",null,"1606-XLS480E",null,null,"A"]
["1 phase 120/230VAC / 24VDC 40A",null,"1606-XLS960E",null,null,"A"]
["UPS 24VDC ",null,"1606-XLS240-UPS",null,null,"A"]
["Battery",null,"1606-XLSBATASSY2",null,null,"A"]
["Transformer : 400V AC Primary"]
["1 phase 380-400-416V / 230V 1000VA","Rockwell","1497B-A11-M15-0-N","- protection with 140MT\n- to be defined according the input voltage",null,"A"]
["1 phase 380-400-416V / 230V 1500VA",null,"1497B-A12-M15-0-N",null,null,"A"]
["1 phase 380-400-416V / 230V 2000VA",null,"1497B-A13-M15-0-N",null,null,"A"]
["1 phase 380-400-416V / 230V 3000VA",null,"1497B-A14-M15-0-N",null,null,"A"]
["Transformer : 480V AC Primary"]
["1 phase 240x480V / 120-230V 1000VA","Rockwell","1497B-A11-M14-0-N","- protection with 140MT\n- to be defined according the input voltage",null,"A"]
["1 phase 240x480V / 120-230V 1500VA",null,"1497B-A12-M14-0-N",null,null,"A"]
["1 Phase  240x480V / 120-230V 2000VA",null,"1497B-A13-M14-0-N",null,null,"A"]
["1 phase 240x480V / 120-230V 3000VA",null,"1497B-A14-M14-0-N",null,null,"A"]
["Transformer : 600V AC Primary"]
["1 phase 600-575-550V / 120-230V 1000VA","Rockwell","1497B-A11-M11-0-N","- protection with 140MT\n- to be defined according the input voltage",null,"A"]
["1 phase 600-575-550V / 120-230V 2000VA",null,"1497B-A13-M11-0-N",null,null,"A"]
["1 phase 600-575-550V / 120-230V 3000VA",null,"1497B-A14-M11-0-N",null,null,"A"]

{"sheet":"18.MCC Panel","index":13,"n_rows":74,"n_cols":8,"rows_kept":74,"cut":false,"hidden":false,"merged":[[34,0,34,7],[4,0,9,0],[10,0,15,0],[16,0,21,0],[22,0,27,0],[28,0,33,0],[0,0,0,6],[66,0,73,0],[65,0,65,7],[60,0,60,7],[43,0,43,7],[3,0,3,7]]}
["MCC PANEL",null,null,null,null,null,null,{"$error":"#VALUE!"}]
[]
["Length \n(mm)","Designation","Supplier","Reference\nfor Saint-Gobain","Quantity","Remark","Comment","Revision"]
["Process "]
[800,"PaneL 2000x800x600","Rittal","VX 8806.000",1,"- Width to be selected according the final layout\n- Typical cabinet 2000x1200x600",null,"A"]
[null,"Comfort Handle","Rittal","VX 8618.250",1,null,null,"A"]
[null,"Semi cylinder for Handle Key N°3524E","Rittal","SZ 2467.000",1,null,null,"A"]
[null,"Base/Plinth: Corner pieces, front and rear pieces\n 200mm Height, 800 Width","Rittal","VX 8660.023",1,null,null,"A"]
[null,"Base/Plinth: Side pieces\n 200mm Height, 600 Width","Rittal","VX 8660.043",1,null,null,"A"]
[null,"Section for cable entry","Rittal","VX 8618.801",1,null,null,"A"]
[1000,"Panel 2000x1000x600","Rittal","VX 8006.000",1,"- Width to be selected according the final layout\n- Typical cabinet 2000x1200x600",null,"A"]
[null,"Comfort Handle","Rittal","VX 8618.250",1,null,null,"A"]
[null,"Semi cylinder for Handle Key N°3524E","Rittal","SZ 2467.000",1,null,null,"A"]
[null,"Base/Plinth: Corner pieces, front and rear pieces\n 200mm Height, 1000 Width","Rittal","VX 8660.024",1,null,null,"A"]
[null,"Base/Plinth: Side pieces\n 200mm Height, 600 Width","Rittal","VX 8660.043",1,null,null,"A"]
[null,"Section for cable entry","Rittal","VX 8618.802",1,null,null,"A"]
[1200,"Panel 2000x1200x600 mm","Rittal","VX 8206.000",1,"- Width to be selected according the final layout\n- Typical cabinet 2000x1200x600",null,"A"]
[null,"Comfort Handle","Rittal","VX 8618.250",1,null,null,"A"]
[null,"Semi cylinder for Handle Key N°3524E","Rittal","SZ 2467.000",1,null,null,"A"]
[null,"Base/Plinth: Corner pieces, front and rear pieces\n 200mm Height, 1200 Width","Rittal","VX 8660.025",1,null,null,"A"]
[null,"Base/Plinth: Side pieces\n 200mm Height, 600 Width","Rittal","VX 8660.043",1,null,null,"A"]
[null,"Section for cable entry","Rittal","VX 8618.803",1,null,null,"A"]
["PLC","Panel 2000x600x600","Rittal","VX 8606.000",1,null,null,"A"]
[null,"Comfort Handle","Rittal","VX 8618.250",1,null,null,"A"]
[null,"Semi cylinder for Handle Key N°3524E","Rittal","SZ 2467.000",1,null,null,"A"]
[null,"Base/Plinth: Corner pieces, front and rear pieces\n 200mm Height, 600 Width","Rittal","VX 8660.022",1,null,null,"A"]
[null,"Base/Plinth: Side pieces\n 200mm Height, 600 Width","Rittal","VX 8660.043",1,null,null,"A"]
[null,"Section for cable entry","Rittal","VX 8618.800",1,null,null,"A"]
["Common","Side panels","Rittal","VX 8106.245",1,"- mandatory for any package",null,"A"]
[null,"Baying cover","Rittal","TS 8800.865",1,"- only if case of assembly","- 1 for 2 panels","A"]
[null,"Baying Connectors (External, 6 pieces)","Rittal","VX 8617.502",1,"- only if case of assembly","- 1 for 2 panels","A"]
[null,"Baying Brackets (Internal, 6 pieces)","Rittal","VX 8617.500",1,"- only if case of assembly","- 1 for 2 panels","A"]
[null,"Mounting plate Infill","Rittal","VX 4591.700",1,"- only if case of assembly","- 1 for 2 panels","A"]
[null,"Combinaison angle (Lifting ring)","Rittal","TS4540.000",1,"- only if case of assembly",null,"A"]
["Network / IT panel"]
[null,"Network enclosure 2000x600x1000","Rittal","VX 5308.113",1,"- Network panel front and back access doors",null,"A"]
[null,"Side panel","Rittal","VX 8100.245",1,"- Side panel VX 2000x1000",null,"A"]
[null,"Base/Plinth: Corner pieces, front and rear pieces\n 100mm Height, 600 Width","Rittal","VX 8660.002",1,null,null,"A"]
[null,"Base/Plinth: Side pieces\n100mm Height, 1000 Width","Rittal","VX 8660.035",1,null,null,"A"]
[null,"Slide rails, heavy-duty","Rittal","VX 5302.031",2,"- One per server",null,"A"]
[null,"Socket strips 19\"","Rittal","DK 7000.630",2,null,null,"A"]
[null,"Cam lock N° 3524E for box","Rittal","SZ 2430.000",2,"- 1 per door",null,"A"]
[null,"Shelf 2U","Rittal","DK 7119.400",1,null,null,"A"]
["Air cooling and Fans "]
[null," Blue e+ wall-mounted cooling units, 110-240VAC 1Ph, 380-480VAC 1.6KW","Rittal","SK 3185.830",1,"According calculation",null,"A"]
[null," Blue e+ wall-mounted cooling units, 110-240VAC 1Ph, 380-480VAC 2KW","Rittal","SK 3186.930",1,"According calculation",null,"A"]
[null," Blue e+ wall-mounted cooling units, 110-240VAC 1Ph, 380-480VAC 2.6KW","Rittal","SK 3187.930",1,"According calculation",null,"A"]
[null," Blue e+ wall-mounted cooling units, 380-480VAC 3Ph 2.6KW","Rittal","SK 3188.940",1,"According calculation",null,"A"]
[null," Blue e+ wall-mounted cooling units, 380-480VAC 3Ph 5.8KW","Rittal","SK 3189.940",1,"According calculation",null,"A"]
[null,"Cooling units, SK 80W 100-240V","Rittal","SK 3201.200",1,"Operator panels and IT boxes",null,"A"]
[null,"Cooling fans 225/245m3/h 115VAC","Rittal","SK 3241.710",1,"According calculation",null,"A"]
[null,"Cooling fans 225/245m3/h 230VAC","Rittal","SK 3241.700",1,"According calculation",null,"A"]
[null,"Outlet filter to be installed with fans 225/245m3/h","Rittal","SK 3239.300",1,"According calculation",null,"A"]
[null,"Cooling fans 540/559m3/h 115VAC","Rittal","SK 3243.710",1,"According calculation",null,"A"]
[null,"Cooling fans 540/559m3/h 230VAC","Rittal","SK 3243.700",1,"According calculation",null,"A"]
[null,"Outlet filter to be installed with fans 540/559m3/h","Rittal","SK 3240.300",1,"According calculation",null,"A"]
[null,"Cooling fans 700/770m3/h 115VAC","Rittal","SK 3244.710",1,"According calculation",null,"A"]
[null,"Cooling fans 700/770m3/h 230VAC","Rittal","SK 3244.700",1,"According calculation",null,"A"]
[null,"Outlet filter to be installed with fans 700/770m3/h","Rittal","SK 3243.300",1,"According calculation",null,"A"]
[null,"Thermostat to be used with fan","Rittal","SK 3110.000",1]
["Light"]
[null,"Led system light wit motion sensor, 110-240VAC ","Rittal","SZ 2500.300",1,null,null,"A"]
[null,"Light connection cable ","Rittal","SZ 2500.400",1,null,null,"A"]
[null,"Light connection cable UL approvals","Rittal","SZ 2500.500",1,null,null,"A"]
[]
["UL-CSA PANEL - ISOLATOR HANDLE PANEL"]
[119.5,"PaneL 2000x119,5x600","Rittal","8950.060",1,null,"on each panel","A"]
[null,"Interconnecting rods - 600 width","Rittal","4916.000",1,null,"on each panel","A"]
[null,"Interconnecting rods - 800 width","Rittal","4918.000",1,null,"on each panel","A"]
[null,"Interconnecting rods - 1200 width","Rittal","4920.000",1,null,"on each panel","A"]
[null,"Adjacent door latch for single-door enclosures","Rittal","4911.000",1,null,"on each panel","A"]
[null,"Adjacent door latch for two-door enclosures","Rittal","4911.100",1,null,"on each panel","A"]
[null,"Operating mechanism","Rittal","4912.000",1,null,"in every fourth adjacent enclosure.","A"]
[null,null,"Rittal",null,1]

{"sheet":"19.Local Boxes","index":14,"n_rows":11,"n_cols":7,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,0,0,5]]}
["Local boxes (CRB)",null,null,null,null,null,{"$error":"#VALUE!"}]
[]
["Designation","Supplier","Reference","Quantity","Remark","Comment","Revision"]
["Bus enclosures KX 380x300x155","Rittal","KX 1576.000",1,null,null,"A"]
["AX Box with mounting plate 380x300x210mm","Rittal","AX 1031.000",1,null,null,"A"]
["AX Box with mounting plate 600x600x210mm","Rittal","AX 1060.000",1,null,null,"A"]
["AX Box with mounting plate 800x400x250mm","Rittal","AX 1094.000",1,null,null,"A"]
["AX Box with mounting plate 800x600x300mm","Rittal","AX 1055.000",1,null,null,"A"]
["Outlet filter Standard","Rittal","SK 3237.300",2,"Per CRB",null,"A"]
["Mini-comfort handle AX","Rittal","AX 2537.100",null,"According locks quantity",null,"A"]
["Semi cylinder for Handle lock-insert locking N° 3524 E for AX","Rittal","SZ 2467.000",null,"According locks quantity",null,"A"]

{"sheet":"20.Bus bar","index":15,"n_rows":17,"n_cols":6,"rows_kept":17,"cut":false,"hidden":false,"merged":[[0,0,0,4]]}
["Bus Bar",null,null,null,null,{"$error":"#VALUE!"}]
[]
["Designation","Supplier","Reference","Remark","Comment","Revision"]
["Base tray for RiLine busbar systems L:500mm","Rittal","SV 9340,100",null,null,"A"]
["Base tray for RiLine busbar systems L:700mm","Rittal","SV 9340,110",null,null,"A"]
["Base tray for RiLine busbar systems L:900mm","Rittal","SV 9340,120",null,null,"A"]
["Base tray for RiLine busbar systems L:1100mm","Rittal","SV 9340,130",null,null,"A"]
["Base tray for RiLine busbar systems L:2400mm","Rittal","SV 9340,170",null,null,"A"]
["Cover section for RiLine busbar systems L:700mm","Rittal","SV 9340,200",null,null,"A"]
["Cover section for RiLine busbar systems L:1100","Rittal","SV 9340,210",null,null,"A"]
["End cover","Rittal","SV 9340,070",null,null,"A"]
["Connection adaptor until 63A  (to supply circuit breaker distribution)","Rittal","SV 9342.210",null,null,"A"]
["Connection adaptor 125A","Rittal","SV 9342,220",null,null,"A"]
["Connection adaptor 250A","Rittal","SV 9342,250",null,null,"A"]
["Connection adaptor 800A","Rittal","SV 9342,280",null,null,"A"]
["Connection adaptor 1200A","Rittal","SV 9342,320",null,null,"A"]
["Busbar support for flat copper busbars","Rittal","SV 9340,050","- space between support according table below",null,"A"]

{"sheet":"21.Terminal Block","index":16,"n_rows":33,"n_cols":7,"rows_kept":33,"cut":false,"hidden":false,"merged":[[3,0,3,6],[10,0,10,6],[14,0,16,0],[4,0,6,0],[7,0,9,0],[4,3,9,3],[11,0,13,0],[11,3,25,3],[0,0,0,5],[29,0,29,6],[27,3,28,3],[17,0,19,0],[20,0,22,0],[23,0,25,0],[26,0,26,6]]}
["Terminal Block Selection",null,null,null,null,null,{"$error":"#VALUE!"}]
[]
["Section\n(mm²)","Series","Specification","Supplier","Reference","Remark","Revision"]
["Control Phoenix Contact"]
["0,14 to 4²","PT 2,5 QUATTRO","Grey","Phoenix Contacts",3209578,null,"A"]
[null,"PT 2,5 QUATTRO-PE","Green/Yellow",null,3209594,null,"A"]
[null,"D-ST 2,5 QUATTRO","End cover",null,3030514,null,"A"]
["4 to 6²","PT 4 QUATTRO","Grey",null,3211797,null,"A"]
[null,"PT 4 QUATTRO-PE","Green/Yellow",null,3211809,null,"A"]
[null,"D-PT 4 QUATTRO","End cover",null,3208979,null,"A"]
["Power Phoenix Contact"]
["UP TO 2,5²","PT 2,5","Grey","Phoenix Contacts",3209510,null,"A"]
[null,"PT 2,5-PE","Green/Yellow",null,3209536,null,"A"]
[null,"D-ST 2,5","End cover",null,3030417,null,"A"]
["4 to 6²","PT 4","Grey",null,3211757,null,"A"]
[null,"PT 4-PE","Green/Yellow",null,3211766,null,"A"]
[null,"D-ST 4","End cover",null,3030420,null,"A"]
["6 to 10²","PT 6","Grey",null,3211813,null,"A"]
[null,"PT 6-PE","Green/Yellow",null,3211822,null,"A"]
[null,"D-PT 6","End cover",null,3212044,null,"A"]
["10 to 16²","PT 10","Grey",null,3212120,null,"A"]
[null,"PT 10-PE","Green/Yellow",null,3212131,null,"A"]
[null,"D-PT 10","End cover",null,3212057,null,"A"]
["16 to 25²","PT 16 N","Grey",null,3212138,null,"A"]
[null,"PT 16 N-PE","Green/Yellow",null,3212147,null,"A"]
[null,"D-PT 16 N","End cover",null,3212060,null,"A"]
["Special for cutter"]
["0,14 to 4²","PT 2,5-QUATTRO-MT ","Grey","Phoenix Contacts",3210172,null,"A"]
[null,"D-ST 2,5 QUATTRO-MT ","End cover",null,3038590,null,"A"]
["Power NVENT ERIFLEX"]
["10-120mm²  Max 250Amps","SBLL250",null,"NVENT ERIFLEX",561132,null,"A"]
["16-400mm²  Max 500Amps","SBLL500",null,"NVENT ERIFLEX",561134,null,"A"]
["25-300mm² x2   Max 800Amps","SBLL800",null,"NVENT ERIFLEX",561136,null,"A"]

{"sheet":"30.Burner","index":17,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,0,0,7]]}
["Burner equipment and instruments (Classic)"]
[]
["Designation","Signal","Supplier","Reference","Remark","Range","Comment","Revision"]
["Flame scanner","Power : 24 VDC Flame strangth Signal : 4-20mA","Durag","D-LX 110 UL or                 D-LX 110 UA",null,null,null,"A"]
["Burner turbine meter","Modbus RTU","RMG","TME400-VC","Not SIL-rated so can be used only on burners where gas flow measurement is not part of the ratio control handled by safety PLC",null,"- Electronic Turbine Gas Flow Meter\n- Volume Compensator (Temperature and Pressure)","A"]
["Burner exit temperature thermocouples","Type J or Type K","Endress+Hauser","Omnigrad M TC12  Omnigrad S TAF16\nTC13","SIL compliant head transmitter TMT82 to be used",null,"For high temperature interlocks and displaying on SCADA.","A"]
["Combustion air temperature transmitters","4-20mA","Endress+Hauser"," Part number to be defined by burner supplier.\nMust be approved by S-G.","SIL compliant head transmitter TMT82 to be used",null,"For temperature compensation of the combustion air.","A"]
["Combustion air pressure transmitters","4-20mA","Endress+Hauser"," Part number to be defined by burner supplier.\nMust be approved by S-G.",null,null,"- For controlling of the comb. air pressure with VFD.\n'- SIL2/SIL3","A"]
["Solenoid valve","24 VDC (power)","Asco or Festo",null,null,null,"For instrument air, process air, combustion air.","A"]
["Gas pressure switches","24 VDC","Fema or Honeywell\nDungs","Dungs model TBC",null,null,"For low gas pressure, high gas pressure ans leak test.","A"]
["Air pressure switches","24 VDC","Honeywell\nDungs","Kromschroder DG\nDungs model TBC",null,null,"For process and combustion air pressure switches.","A"]
["Pilot gas valves","24 VDC","Honeywell","Kromschroder VAS",null,null,"Pilot gas train safety shut off valves.","A"]
["Safety Shut Off Valves","24 VDC (power and feedback signals)","Honeywell\nDungs","Maxon 8000\nDungs model TBC","Pneumatic, requires instrumentation air.",null,"Main gas train safety shut off valves. ","A"]
["Actuated Valves","24 VDC (power and feedback signals)","Schubert&Salzer","Type 8231",null,null,"Gas flow regulation","A"]

{"sheet":"31.Burner Fiberizing","index":18,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":true,"merged":[[0,0,0,7]]}
["Burner for fiberizing machine"]
[]
["Designation","Signal","Supplier","Reference","Remark","Range","Comment","Revision"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]

{"sheet":"32.Burner SBM","index":19,"n_rows":14,"n_cols":8,"rows_kept":14,"cut":false,"hidden":true,"merged":[[0,0,0,7]]}
["SBM"]
[]
["Designation","Signal","Supplier","Reference","Remark","Range","Comment","Revision"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]
[null,null,null,null,null,null,null,"A"]

{"sheet":"40.Siemens-CPU","index":20,"n_rows":10,"n_cols":4,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Siemens - CPU Selection",null,null,{"$error":"#VALUE!"}]
[]
["Designation","Reference","Comments","Revision"]
["CPU 1515F-2PN","6ES7515-2FN03-0ABA0","use for general applications","A"]
["CPU 1515TF-2PN","6ES7515-2UN03-0AB0","use for cutter","v"]
["CPU 1517TF-3PN","6ES7517-3UQ10-0ABA0","use for short cycle time \ni.e. W.E.T","A"]
["Memory Card 24 MB"," 6ES7954-8LF04-0AA0","for CPU 1512SP F-1 PN ","A"]
["Memory Card 256 MB","6ES7954-8LL04-0AA0","for 1515 and 1517 CPUs","A"]
["CPU 1500 Mounting Rail","6ES7590-1AB60-0AA0","To be order with 1500 CP","A"]
["CPU 1512SP F-1 PN ","6ES7512-1SM03-0AB0","use for burner control  / small auxiliary applications","A"]

{"sheet":"41.Siemens-ET200SP","index":21,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[3,3,4,3],[3,0,4,0],[0,0,0,3]]}
["Siemens - ET200SP Selection",null,null,null,{"$error":"#VALUE!"}]
[]
["Type","Designation","Reference","Comments","Revision"]
["Interface module","Interface module IM155 High Feature","6ES7155-6MU01-0CN0","To be ordered together","A"]
[null,"SIMATIC ET 200SP, BusAdapter BA 2xRJ45","6ES7193-6AR00-0AA0",null,"A"]
["Terminals","DI / DO spring load terminals for new group","6ES7193-6BP20-0DA0 ",null,"A"]
[null,"DI / DO spring load terminals bridged","6ES7193-6BP20-0BA0 ",null,"A"]
[null,"AI / AO spring load terminals for new group","6ES7193-6BP40-0DA1 ",null,"A"]
[null,"AI / AO spring load terminals bridged.","6ES7193-6BP40-0BA1 ",null,"A"]
["Standard","8 DI 24VDC high feature","6ES7131-6BF00-0CA0 ",null,"A"]
[null,"8 DO 24VDC 0.5A high feature","6ES7132-6BF01-0CA0 ",null,"A"]
[null,"4 DO 24VDC 2A high feature","6ES7132-6BD21-0CA0","Use only if necessary to control high current consumer","A"]
[null,"4 AI 2/4 wire. standard +/- 20mA,4-20mA","6ES7134-6GD01-0BA1",null,"A"]
[null,"4 A0 U/I standard +/- 20mA, +-10V","6ES7135-6HD00-0BA1 ",null,"A"]
[null,"4 AI RTD high feature","6ES7134-6JD00-0CA1",null,"A"]
["Communication","RS422/485/232 communication module","6ES7137-6AA00-0BA0",null,"A"]
["Weighing","SIWAREX WP351","7MH4138-6BA00-0CU0",null,"A"]
[null,"SIWAREX spring load terminals for new group","6ES7193-6BP00-0DU0",null,"A"]
[null,"SIWAREX spring load terminals bridged","6ES7193-6BP00-0BU0 ",null,"A"]
["Fail Safe","8 DI SAFE 24VDC","6ES7136-6BA01-0CA0 ",null,"A"]
[null,"4 DO SAFE 24VDC/2A","6ES7136-6DB00-0CA0 ",null,"A"]
[null,"4 AI SAFE 0(4)..20mA","6ES7136-6AA00-0CA1",null,"A"]

{"sheet":"42.Siemens-ET200SP DOL","index":22,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[[24,0,24,5],[0,0,0,4]]}
["Siemens - ET200SP DOL",null,null,null,null,{"$error":"#VALUE!"}]
[]
["Type","Designation","Motor power","Reference","Comments","Revision"]
["Reservation module","cover",null,"6ES7133-6CV15-1AM0","On ET200SP motor system a reservation module should be\nmounted before the first base unit","A"]
[null,"Base unit",null,"6ES7193-6BP20-0DA0",null,"A"]
["Base Unit","BU30-MS1\n (new 24VDC & 500VAC groups)",null,"3RK1908-0AP00-0AP0","First base unit for 400VAC and 24Vdc supplies","A"]
[null,"BU30-MS4\n (24VDC & 500VAC taken from the left base unit)",null,"3RK1908-0AP00-0DP0",null,"A"]
[null,"BU30-MS2\n(new 500VAC group)",null,"3RK1908-0AP00-0CP0",null,"A"]
[null,"BU30-MS3\n(new 24VDC group)",null,"3RK1908-0AP00-0BP0",null,"A"]
["Standard Motor starter","ET200SP motor starter 0,1 - 0,4A","0,15KW","3RK1308-0AA00-0CP0",null,"A"]
[null,"ET200SP motor starter 0,3A - 1A","0,25KW","3RK1308-0AB00-0CP0",null,"A"]
[null,"ET200SP motor starter 0,9A - 3A","1,1KW","3RK1308-0AC00-0CP0",null,"A"]
[null,"ET200SP motor starter 2,8A - 9A","4KW","3RK1308-0AD00-0CP0",null,"A"]
["Standard Reverse Motor starter","ET200SP motor reverse starter 0,1 - 0,4A","0,15KW","3RK1308-0BA00-0CP0",null,"A"]
[null,"ET200SP motor reverse starter 0,3A - 1A","0,25KW","3RK1308-0BB00-0CP0",null,"A"]
[null,"ET200SP motor reverse starter 0,9A - 3A","1,1KW","3RK1308-0BC00-0CP0",null,"A"]
[null,"ET200SP motor reverse starter 2,8A - 9A","4KW","3RK1308-0CD00-0CP0",null,"A"]
["Fail Safe Motor starter","ET200SP Safe motor starter 0,3A - 1A","0,25KW","3RK1308-0CB00-0CP0",null,"A"]
[null,"ET200SP Safe motor starter 0,9A - 3A","1,1KW","3RK1308-0CC00-0CP0",null,"A"]
[null,"ET200SP Safe motor starter 2,8A - 9A","4KW","3RK1308-0CD00-0CP0",null,"A"]
["Fail Safe Reverse Motor starter","ET200SP Safe motor reverse starter 0,3A - 1A","0,25KW","3RK1308-0DB00-0CP0",null,"A"]
[null,"ET200SP Safe motor reverse starter 0,9A - 3A","1,1KW","3RK1308-DC00-0CP0",null,"A"]
[null,"ET200SP Safe motor reverse starter 2,8A - 9A","4KW","3RK1308-0DD00-0CP0",null,"A"]
[]
["You have to use https://mall.industry.siemens.com/tstcloud/#/Start to confirm your ET200SP DOL configuration"]

{"sheet":"60.Rockwell-CPU","index":23,"n_rows":9,"n_cols":5,"rows_kept":9,"cut":false,"hidden":true,"merged":[[0,0,0,4]]}
["Rockwell - CPU Selection"]
[]
["Designation","Reference","Comments","Certification","Revision"]
["Rack","1756-A7",null,"CE / c-UL-us","D"]
["Power Supply","1756-PB50",null,"CE / c-UL-us","D"]
["CPU","1756-L82ES","up to PL \"d\"","CE / c-UL-us","D"]
["Safety Partner","1756-L8SP","to achieved PL \"e\"","CE / c-UL-us","D"]
["Memory card","1784-SD1",null,"CE / c-UL-us","D"]
["Ethernet card","1756-EN3TR",null,"CE / c-UL-us","D"]

{"sheet":"61.Rockwell-Point IO","index":24,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":true,"merged":[[0,0,0,5]]}
["Rockwell - Point I/O Selection"]
[]
["Type","Designation","Reference","Comments","Certification","Revision"]
["Interface module",null,"1734-AENTR","Ethernet/IP module","CE / c-UL-us","A"]
["Terminals","Wiring Base","1734-TBS","spring clamp terminals","CE / c-UL-us","A"]
[null,"Removable block","1734-RTBS","spring clamp terminals","CE / c-UL-us","A"]
["Standard","4x Digital inputs","1734-IB4D",null,"CE / c-UL-us","A"]
[null,"4x Digital outputs","1734-OB4E",null,"CE / c-UL-us","A"]
[null,"2x analog inputs 4-20mA","1734-IE2C",null,"CE / c-UL-us","A"]
[null,"2x analog inputs +/-10V","1734-IE2V",null,"CE / c-UL-us","A"]
[null,"2x analog outputs 4-20mA\n+-10V","1734-OE2C",null,"CE / c-UL-us","A"]
[null,"2x analog outputs +/-10V","1734-OE2V",null,"CE / c-UL-us","A"]
[null,"2x RTD","1734-IR2",null,"CE / c-UL-us","A"]
["Modbus","Modbus communication module","ILX34-MBS485","from Prosoft","CE / c-UL-us","D"]
["Weighing","Weigh Scale module","HI1734-WS","from Hardy","!!!!!!!!Lk/","D"]
["Fail Safe","4/8x Fail safe digital inputs","1734-IB8S","need 2x terminal base TBS","CE / c-UL-us","D"]
[null,"8x Fail safe digital outputs","1734-OB8S","need 2x terminal base TBS","CE / c-UL-us","D"]
[null,"4x Fail safe analogue input","1734-IE4S","need 2x terminal base TBS","CE / c-UL-us","D"]
["Accessories","Field ower Distributor module","1734-FPD",null,"CE / c-UL-us","A"]
[null,"Expansion power module","1734-EP24DC",null,"CE / c-UL-us","A"]